[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Current

- To: femm@yahoogroups.com
- Subject: Current
- From: "brian_hawes" <b.hawes1@physics.ox.ac.uk>
- Date: Thu, 18 Jul 2002 13:50:41 -0000
- User-agent: eGroups-EW/0.82

    Hi, I'm new here, so be patient if I've missed anything.
    I have started to use FEMM to look at current distribution within the
    turns of a coil. Skin effect and Proximity effect. I have some
    problem reconciling the current density specified in the original
    materials property (for the copper) and the total current calculated
    by integrating over the area of the wire cross section in the result.
    Can someone enlighten me please?
    Brian Hawes

- Follow-Ups:
  - Re: [femm] Current
    - From: Keith Gregory <k.gregory@lboro.ac.uk>

- Prev by Date: Force Calculus Methods
- Next by Date: Re: [femm] Current
- Previous by thread: Re: Force Calculus Methods
- Next by thread: Re: [femm] Current
- Index(es):
  - Date
  - Thread