[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Call to triangle unsucessful after import of DXF

- To: <femm@yahoogroups.com>
- Subject: Re: [femm] Call to triangle unsucessful after import of DXF
- From: "Eric Vogels" <eric.vogels@telia.com>
- Date: Fri, 13 Dec 2002 19:29:07 +0100
- References: <atacjq+v3ob@eGroups.com>

Hi Stefan. I'm not a specialist but I did the same asyou did (import) and had to overcome some problems as well. If you send me the model I'll take a look. eric.vogels@telia.com Eric. ----- Original Message ----- From: stefannilsson2003 <stefan.a.nilsson@metso.com> To: femm@yahoogroups.com Sent: Thursday, December 12, 2002 5:13 PM Subject: [femm] Call to triangle unsucessful after import of DXF `Hello, David helped me to fix femm 3.2 so that I can import DXF from Autocad R14. But when I try to create mesh I get the message:Call to triangle unsucessful. What is the problem? My model consists of permanetmagnets placed on a steel plate with R 455 mm. It's for a magnet drum. Help appreciated. I can send model if needed. Regards Stefan Nilsson` `Your useof Yahoo! Groups is subject to the Yahoo! Terms of Service.`

- References:
  - Call to triangle unsucessful after import of DXF
    - From: "stefannilsson2003 <stefan.a.nilsson@metso.com>" <stefan.a.nilsson@metso.com>

- Prev by Date: Re: [femm] General question and/or proposition for the circuit property and global variable
- Next by Date: Femm releases 3.3 - 3.2
- Previous by thread: Re: [femm] Call to triangle unsucessful after import of DXF
- Next by thread: How to get the leakage inductance when very bad coupling.
- Index(es):
  - Date
  - Thread