[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Permanent magnet operating point

- To: femm@yahoogroups.com
- Subject: Permanent magnet operating point
- From: "tano1938" <rgarritano@comcast.net>
- Date: Fri, 09 May 2003 17:34:22 -0000
- User-agent: eGroups-EW/0.82

    What,s the best way to get the permanent magnet operating point for a
    magnetic circuit using femm. I've been using the integral of B over
    the block (magnet), dividing this by the volume to get the average B
    and then using this average B with the the magnet data curve and
    coercivity to get H. Is there a better or an easier way.

    Thanks for your help

- Follow-Ups:
  - Re: Permanent magnet operating point
    - From: "David Meeker" <dmeeker@ieee.org>

- Prev by Date: Re: [femm] passing values between Lua scripts
- Next by Date: Re: [femm] Lua script
- Previous by thread: Re: [femm] TetGen, a 3D tetrahedral mesh generator
- Next by thread: Re: Permanent magnet operating point
- Index(es):
  - Date
  - Thread