[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# [FEMM] modeling coils???

- To: "'femm@list.foster-miller.net'" <femm@list.foster-miller.net>
- Subject: [FEMM] modeling coils???
- From: Dobler Daniel <dobler.daniel@rw.hirschmann.at>
- Date: Mon, 29 Mar 2004 12:10:58 +0200
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: FEMM mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- Reply-to: FEMM mailing list <femm@list.foster-miller.net>

Hi

I think you forgot to put some turns around the pure iron core. You just have to add the series circuit property to both copper parts around the core. Be sure to give one side of the copper a negative amount of turns.

Daniel

- Prev by Date: RE: [FEMM] modeling coils???
- Next by Date: RE: [FEMM] modeling coils???
- Previous by thread: [FEMM] Inductance of lap wnding
- Next by thread: RE: [FEMM] modeling coils???
- Index(es):
  - Date
  - Thread