[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] slip frequency....I need help

- To: femm@yahoogroups.com
- Subject: Re: [femm] slip frequency....I need help
- From: riad kechrpud <r_kechroud@yahoo.fr>
- Date: Fri, 18 Apr 2003 15:11:48 +0200 (CEST)
- In-reply-to: <b7oi1o+5sn7@eGroups.com>

One way to simulate induction operation is to impose a frequency egal to gf (where g is the slip and the f is the power system frequency) either in the sator and in the rotor. This is called a static ou qusi static rotor model. It is like suppplying the induction motor with a power system having a frequency equal to gf while keeping the rotor blocked.

There is some similitudes with Steinmeitz model of the induction motor where the load is taken into account by dividing the rotor resistance by the slip.

Do You Yahoo!? -- Une adresse @yahoo.fr gratuite et en français !
Testez le nouveau Yahoo! Mail

- References:
  - slip frequency....I need help
    - From: "linearmotor77" <linearmotor77@yahoo.co.kr>

- Prev by Date: slip frequency....I need help
- Next by Date: Vector plots + "zoomier"
- Previous by thread: slip frequency....I need help
- Next by thread: Vector plots + "zoomier"
- Index(es):
  - Date
  - Thread