[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# TO OBILGIN

- To: femm@yahoogroups.com
- Subject: TO OBILGIN
- From: "mercedes sampere" <m_veinti2@hotmail.com>
- Date: Thu, 25 Oct 2001 17:59:24 -0300
- Bcc:

`Hi Obilgin!
I've read your last mails and I would be gratefull if you could help me. I'm studing leakage reactance for a motor, too, but I can't realise how to set the coils.
I've simulated it with femm but I think there's something wrong with the wound because flux is too low.
I send you my model.
It's an induction motor:
Usefull power: 88.1kW
Tension: 380/660 V
Synchronous speed: 1500 rpm
Frecuency: 50 Hz
Number of phases: 3
Two pairs of poles
Power factor: 0.89
Sliding coefficient: 0.0133
Current per phase(stator): 88.8 A
Number of slots(stator): 48
Current per phase(rotor): 370 A
Number of slots(rotor): 36
Double layer(stator and rotor)
Overlaid wound.
Wound coefficients:
stator: k= 0.925
rotor: k= 0.96`
`Maybe you can send me your model to have an idea how to put the coils even though it is not an induction motor, or if you want to you can check my model.
Thank you very much.
Mercedes`
``

    _________________________________________________________________
    Descargue GRATUITAMENTE MSN Explorer en http://explorer.msn.es/intl.asp

Attachment: `motor asinc completo.FEM`
Description: Binary data

- Follow-Ups:
  - Re: [femm] TO OBILGIN
    - From: Alberto Perez <albertoperarnau@yahoo.es>

- Prev by Date: 3 phase cable/animation & thanks
- Next by Date: Re: [femm] complex inductance???
- Previous by thread: Re: [femm] Inductance with permanent magnet
- Next by thread: Re: [femm] TO OBILGIN
- Index(es):
  - Date
  - Thread