[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# why different force??

- To: femm@yahoogroups.com
- Subject: why different force??
- From: "ahmad_m_eid" <ahmad_m_eid@yahoo.com>
- Date: Fri, 05 Sep 2003 03:09:53 -0000
- User-agent: eGroups-EW/0.82

    Dear all
    I use femm in my work in linear generator
    when I trace a path around the stator to find the force by "force
    from stress tensor" I get a value for the force on stator

    when I use the block integration and select all stator blocks anf find
    force from " force via weighted stress tensor" I get another value and
    away from the first value comes from line integral.

    what is the best way to find the force on stator?

    how can one explain these different results?

- Follow-Ups:
  - Re: why different force??
    - From: "David Meeker" <dmeeker@ieee.org>

- Prev by Date: Multiple group membership for nodes
- Next by Date: Re: [femm] Transformer Forward curent and magnetizing current
- Previous by thread: DC motors model
- Next by thread: Re: why different force??
- Index(es):
  - Date
  - Thread