[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Call to triangle unsucessful after import of DXF

- To: femm@yahoogroups.com
- Subject: Call to triangle unsucessful after import of DXF
- From: "stefannilsson2003 <stefan.a.nilsson@metso.com>" <stefan.a.nilsson@metso.com>
- Date: Thu, 12 Dec 2002 16:13:46 -0000
- User-agent: eGroups-EW/0.82

    Hello,
    David helped me to fix femm 3.2 so that I can import DXF from Autocad
    R14. But when I try to create mesh I get the message:Call to triangle
    unsucessful. What is the problem?
    My model consists of permanetmagnets placed on a steel plate with R
    455 mm. It's for a magnet drum.

    Help appreciated. I can send model if needed.

    Regards
    Stefan Nilsson

- Follow-Ups:
  - Re: [femm] Call to triangle unsucessful after import of DXF
    - From: David Meeker <dmeeker@ieee.org>
  - Re: [femm] Call to triangle unsucessful after import of DXF
    - From: "Eric Vogels" <eric.vogels@telia.com>

- Prev by Date: [no subject]
- Next by Date: How to get the leakage inductance when very bad coupling.
- Previous by thread: [no subject]
- Next by thread: Re: [femm] Call to triangle unsucessful after import of DXF
- Index(es):
  - Date
  - Thread