[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Rif: Re: [FEMM] lua to output B field

- To: FEMM mailing list <femm@list.foster-miller.net>
- Subject: Rif: Re: [FEMM] lua to output B field
- From: giovanni.bortolan@sogagroup.com
- Date: Mon, 26 Apr 2004 08:48:40 +0200
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: FEMM mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- Reply-to: FEMM mailing list <femm@list.foster-miller.net>

    Dear Steven,
    you can read .fem file. It is not difficult.
    In .fem file you can find all input data (included the position of all
    nodes).
    If your external dimensions are defined by arcs, you should add a little of
    intelligence to your program.

    Enjoy your lua.
    _______________________________
    ing. G.Bortolan

    Sincro srl
    via Tezze, 3 loc. Cereda
    36073 Cornedo Vicentino (VI)
    ITALY
    Tel: (++39) 0445 450 500
    Fax: (++39) 0445 446 190
    e-mail: Giovanni.Bortolan@sogagroup.com
                   tecnico.sincro@sogagroup.com
    http://www.sogagroup.com

    REA 194515/VI
    Reg. Imp. 20968/VI 116
    P.IVA 01925820241

                          Steven Adeff
                          <adeffs@rpi.edu>                 Per:     femm@list.foster-miller.net
                          Inviato da:                      Cc:
                          femm-bounces@list.foster         Oggetto: Re: [FEMM] lua to output B field
                          -miller.net

                          23/04/2004 18:48
                          Per favore, rispondere a
                          FEMM mailing list

    Ok, I think I'm on my way to getting this to work. Question though, Is
    there a
    way to find the x and y(or r and z) limits of a problem? I'm trying to make
    a
    loop that will go through all the x and y coordinates to get the Bx and By
    values. Right now I have it set to 100(arbitrary) but would like to set it
    to
    whatever the max x and y values are.

    thanks!
    --
    Steven Adeff
    ADEFFS@RPI.EDU
    Graduate, Electric Power Engineering
    Rensselaer Polytechnic Institute - Troy, NY

    On Thursday 22 April 2004 12:31 pm, Steven Adeff wrote:
    > is it possible to use LUA to ouput the B field values and the x,y
    > coordinates for a whole analysis area into a text file?
    _______________________________________________
    FEMM mailing list
    FEMM@list.foster-miller.net
    http://femm.foster-miller.net/mailman/listinfo/femm

- Prev by Date: [FEMM] force output format?
- Next by Date: [FEMM] Accuracy error
- Previous by thread: [FEMM] force output format?
- Next by thread: [FEMM] Accuracy error
- Index(es):
  - Date
  - Thread