[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: Current

- To: femm@yahoogroups.com
- Subject: Re: Current
- From: "brian_hawes" <b.hawes1@physics.ox.ac.uk>
- Date: Mon, 22 Jul 2002 08:54:09 -0000
- User-agent: eGroups-EW/0.82

    Keith,
    Thanks for the reply. My problem is thus: I have a simple simulation
    of a single curent carrying ring. I have defined the current density
    in the model for the copper. If I simulate at very low frequency,
    such that skin and proximity effects are negligable, then the total
    current, found by using the block integral feature in FemView, is
    what I would expect - J x Area. Now, if I increase the frequency such
    that skin and proximity effects occurr, then the total current,
    measured with FemView appears to fall. I would expect, as you say,
    that the total current would remain constant, and just be
    redistributed.
    Brian

- Follow-Ups:
  - Re: [femm] Re: Current
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: Re: Force Calculus Methods
- Next by Date: torque
- Previous by thread: Re: [femm] Current
- Next by thread: Re: [femm] Re: Current
- Index(es):
  - Date
  - Thread