[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re[2]: [femm] Calculating Shieldi Effectiveness with Femm

- To: David Meeker <femm@egroups.com>
- Subject: Re[2]: [femm] Calculating Shieldi Effectiveness with Femm
- From: V.Petoukhov <stray_current@mtu-net.ru>
- Date: Wed, 24 Jan 2001 06:02:25 +0300
- Priority: Normal
- References: <3A6E026A.D8C96284@foster-miller.com>
- Reply-to: V.Petoukhov <stray_current@mtu-net.ru>

    Hi, I have 2 questions.

    1. In the example sample.fem the "total current" of the aluminum
    shield must be equal zero, but it is not done by "circuit" properties.
    Is it correct? And what a phisical task solved in this example (with
    no "circuit properties" in the aluminum
    shield)?

    2. If it's possible, tell me the addres for downloading
    the student version of Quickfield 3.4a

    Thank you,

    V. Petoukhov

- Follow-Ups:
  - Re: [femm] Calculating Shieldi Effectiveness with Femm
    - From: David Meeker <dmeeker@foster-miller.com>

- References:
  - Re: [femm] Calculating Shieldi Effectiveness with Femm
    - From: David Meeker <dmeeker@foster-miller.com>

- Prev by Date: Re: [femm] Modelling a three phase short circuit of a Synchronous machine.
- Next by Date: leakage flux detection
- Previous by thread: Re: [femm] Calculating Shieldi Effectiveness with Femm
- Next by thread: Re: [femm] Calculating Shieldi Effectiveness with Femm
- Index(es):
  - Date
  - Thread