[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# RE: [femm] electromagnets

- To: <femm@yahoogroups.com>
- Subject: RE: [femm] electromagnets
- From: "Adrian" <adrianw@solid-state-logic.com>
- Date: Mon, 11 Jun 2001 22:32:02 +0100
- Importance: Normal
- In-reply-to: <9g35gf+71bv@eGroups.com>
- Sender: adrianw@solid-state-logic.com

Hi Bruno, I may be missing the point here, but I think you need the axis-symmetric setting. Slice your cylinder along its length, so you have a cross section. Then draw one half of it in FEMMEwith the centre at (FEMME’s) r=0. FEMME will then model your electromagnet as if it were rotated around the r=0 line. Hopethis helps. Adrian -----Original Message----- From: sentto-1333690-439-992293778-adrianwadey=compuserve.com@returns.onelist.com [mailto:sentto-1333690-439-992293778-adrianwadey=compuserve.com@returns.onelist.com]On Behalf Of brvusit@yahoo.it Sent: 11 June 2001 20:18 To: femm@yahoogroups.com Subject: [femm] electromagnets `Hi all.` `I am Bruno Vusini and I am an italian engineer. I have used` `FEMM for my thesis (THANKS DAVE!!). I have used this` `WONDERFUL program for many others problems (motors,` `electromagnetic brakes...) and now...I have a problem...` `Can I model a cylindrical elecromagnet using FEMM? Is there a` `way to transform this problem in a 2D model?` `Thanks to all.` `Bruno.` `Your use of Yahoo! Groups is subject to the Yahoo! Terms of Service.`

- References:
  - electromagnets
    - From: brvusit@yahoo.it

- Prev by Date: Re: electromagnets
- Next by Date: Re: [femm] electromagnets
- Previous by thread: Re: electromagnets
- Next by thread: Re: [femm] electromagnets
- Index(es):
  - Date
  - Thread