[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: Skin effect at nonsinusiodal current

- To: femm@yahoogroups.com
- Subject: Re: Skin effect at nonsinusiodal current
- From: "rob_strandau" <rstrand@ihug.com.au>
- Date: Tue, 02 Apr 2002 14:33:10 -0000
- In-reply-to: <17261.020401@mail.ru>
- User-agent: eGroups-EW/0.82

    --- In femm@y..., V.Petoukhov <V.Petoukhov@m...> wrote:
    > Dear Femm Community,
    > who can help in question of calculating skin and proximity effects in
    > wires and cables at multifrequency case (nonsinusoidal currents).
    > Is any articles, books of software availible?
    >
    > Thank you in advance
    > V. Petoukhov mailto: V.Petoukhov@m...

    A common approximation is to compute SE and PE for each (significant)
    frequency component of the input waveform then add the power loss for
    each component.

    Regards
    Rob

- References:
  - Skin effect at nonsinusiodal current
    - From: V.Petoukhov <V.Petoukhov@mail.ru>

- Prev by Date: Skin effect at nonsinusiodal current
- Next by Date: RE: [femm] Dynamic Animations
- Previous by thread: Skin effect at nonsinusiodal current
- Next by thread: Re: [femm] Skin effect at nonsinusiodal current
- Index(es):
  - Date
  - Thread