[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] current in slot conductors

- To: <femm@yahoogroups.com>
- Subject: Re: [femm] current in slot conductors
- From: "Ivan Slabbert" <ivan_slabbert@msn.com>
- Date: Wed, 3 Sep 2003 12:06:20 +0200
- References: <bj3ovd+b5m7@eGroups.com>

Hallo Ahmad maybe the following LUA code will be usefull to you --set stator currents statorslotarea = 1.058784e-004 turnspercoil = 10 angle = 0 phasecurrent = 30 Jpeak = (((sqrt(2))*phasecurrent*turnspercoil)/statorslotarea)/1000000 -- div 1000000 to convert A/m^2 to MA/m^2 JA=Jpeak*sin(angle) JB=Jpeak*sin(angle -120) JC=Jpeak*sin(angle + 120) modifymaterial("Conductor A1",4,JA) --This machine rotates anti-clockwise modifymaterial("Conductor B1",4,JB) modifymaterial("Conductor C1",4,JC) modifymaterial("Conductor A2",4,(-JA)) modifymaterial("Conductor B2",4,(-JB)) modifymaterial("Conductor C2",4,(-JC)) Ivan Slabbert ----- Original Message ----- From: ahmad_m_eid To: femm@yahoogroups.com Sent: Wednesday, September 03, 2003 5:59 AM Subject: [femm] current in slot conductors `Dear all I work in linear generator field. I want to consider an ac current moving in the coils, so, how can I define this current value?? if the rms value is 20 A and the number of turns/slot = 25 so, the define current will be 20 A or 20*25 in each slot? any suggestion is helpful thanks a lot ahmad`

- References:
  - current in slot conductors
    - From: "ahmad_m_eid" <ahmad_m_eid@yahoo.com>

- Prev by Date: Re: [femm] current in slot conductors
- Next by Date: Re: current in slot conductors
- Previous by thread: Re: [femm] current in slot conductors
- Next by thread: Re: current in slot conductors
- Index(es):
  - Date
  - Thread