[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] current in slot conductors

- To: femm@yahoogroups.com
- Subject: Re: [femm] current in slot conductors
- From: "Prem Kumar C" <prem@bhelrnd.co.in>
- Date: Wed, 03 Sep 2003 10:58:03 +0530
- References: <bj3ovd+b5m7@eGroups.com>

    Ahmad :
    Yes ! You need to specify the slot ampere conductors seperately for the Top conductor & Bottom conductor. If you
    have a 3phase wdg, I suggest you name them R_pos, R_neg and so on..... for simulating the R phase current coming out &
    going into the plane of the paper.

    Prem

    ahmad_m_eid wrote:

    > Dear all
    >
    > I work in linear generator field. I want to consider an ac current
    > moving in the coils, so, how can I define this current value??
    >
    > if the rms value is 20 A and the number of turns/slot = 25
    >
    > so, the define current will be 20 A or 20*25 in each slot?
    >
    > any suggestion is helpful
    >
    > thanks a lot
    >
    > ahmad
    >
    >
    >
    >
    > Your use of Yahoo! Groups is subject to http://docs.yahoo.com/info/terms/

    begin:vcard
    n:Kumar;C.Prem Kumar
    tel;cell:+91 94400 49277
    tel;fax:+91 40 2307 3820
    tel;home:+91 40 2775 1195
    tel;work:+91 40 2388 2347
    x-mozilla-html:FALSE
    org:Electromagnetics Group;BHEL Corp.R&D Division
    adr:;;Vikasnagar P.O,;Hyderabad;Andhra Pradesh;500 093;India
    version:2.1
    email;internet:prem@bhelrnd.co.in
    title:Deputy General Manager
    x-mozilla-cpt:;1888
    fn:C.Prem Kumar
    end:vcard

- References:
  - current in slot conductors
    - From: "ahmad_m_eid" <ahmad_m_eid@yahoo.com>

- Prev by Date: current in slot conductors
- Next by Date: Re: [femm] current in slot conductors
- Previous by thread: current in slot conductors
- Next by thread: Re: [femm] current in slot conductors
- Index(es):
  - Date
  - Thread