[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# leakage flux in the induction motor

- To: femm@egroups.com
- Subject: leakage flux in the induction motor
- From: marki denaro <markiid@yahoo.com>
- Date: Mon, 27 Nov 2000 18:21:25 -0800 (PST)

    how to define the boundary condition & calculate the
    leakage flux using the femm program in 3 phasa squirel
    cage induction motor with
    specification of motor:
    36 slot in stator
    with dimension depth x width = 1.34 x 0.31 inches
    internal diameter of stator = 7 inch
    stamping out diameter of stator = 12.5 inch
    air gap = 0.024 inch

    31 slot in the rotor
    dimension D x W =0.6 x 0.2 inches

    __________________________________________________
    Do You Yahoo!?
    Yahoo! Shopping - Thousands of Stores. Millions of Products.
    http://shopping.yahoo.com/

- Prev by Date: Re: [femm] Metglas square loop BH curves
- Next by Date: ring magnet
- Previous by thread: Re: [femm] LIM
- Next by thread: ring magnet
- Index(es):
  - Date
  - Thread