[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# current in slot conductors

- To: femm@yahoogroups.com
- Subject: current in slot conductors
- From: "ahmad_m_eid" <ahmad_m_eid@yahoo.com>
- Date: Wed, 03 Sep 2003 03:59:41 -0000
- User-agent: eGroups-EW/0.82

    Dear all

    I work in linear generator field. I want to consider an ac current
    moving in the coils, so, how can I define this current value??

    if the rms value is 20 A and the number of turns/slot = 25

    so, the define current will be 20 A or 20*25 in each slot?

    any suggestion is helpful

    thanks a lot

    ahmad

- Follow-Ups:
  - Re: [femm] current in slot conductors
    - From: "Prem Kumar C" <prem@bhelrnd.co.in>
  - Re: [femm] current in slot conductors
    - From: "Ivan Slabbert" <ivan_slabbert@msn.com>
  - Re: current in slot conductors
    - From: "David Meeker" <dmeeker@ieee.org>

- Prev by Date: Transformer Forward curent and magnetizing current
- Next by Date: Re: [femm] current in slot conductors
- Previous by thread: Re: [femm] Transformer Forward curent and magnetizing current
- Next by thread: Re: [femm] current in slot conductors
- Index(es):
  - Date
  - Thread