[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] How to do a B or H "black box" generator in a perpendicular plan to the working

- To: femm@yahoogroups.com
- Subject: Re: [femm] How to do a B or H "black box" generator in a perpendicular plan to the working
- From: David Meeker <dmeeker@ieee.org>
- Date: Tue, 21 Jan 2003 12:21:36 -0500
- References: <b09mv3+gkdf@eGroups.com>
- User-agent: Mozilla/5.0 (Windows; U; Windows NT 5.1; en-US; rv:1.1) Gecko/20020826 MultiZilla/v1.1.22

`jire602000 wrote:`

> `
> Hello every body,`

>     With the Prescribe A boundary condition, B or H can be imposed in
>     the x y (r, z) 2D plan of the study . But how can I make it
>     perpendicular to this plan ? I want it in the same direction as the
>     current of the circuit property of a copper wire for example.

> `This trick can also be achieved by having a current in a cooper wire running in the x y 2D plan and not in the perpendicular plan as usual.`
> `So , I need help and advise !`

`With femm, flux always flows in the plane of the screen and currents flow in the into-the-page direction. You can't solve the sort of problem that you are thinking about with femm, where you want flux to travel in the into-the-page direction.`
`You might be able to solve this problem with Maxwell SV, which Ansoft has recently made available free-of-charge. See http://www.ansoft.com/maxwellsv/ This is a student version of their 2D program, and it's actually quite powerful. There seem to be no mesh size limits--the program just doesn't include what they must consider to be more advanced features, like parametric analyses, transient analyses, etc. It sounds like your type of problem could be addressed by their "eddy axial" solver. For an explanation of the formulation, see: http://www.ansoft.com/support/workshops/emworkshop/Eddy_axial.pdf`
`Dave.`

    --
    David Meeker
    email: dmeeker@ieee.org
    www: http://femm.berlios.de/dmeeker

``

- References:
  - How to do a B or H "black box" generator in a perpendicular plan to the working
    - From: "jire602000 <jire602000@yahoo.com>" <jire602000@yahoo.com>

- Prev by Date: RE: [femm] Need BH curve for chromium steel
- Next by Date: Re: OOT - Parallel FEM Language
- Previous by thread: How to do a B or H "black box" generator in a perpendicular plan to the working
- Next by thread: Inductance variation with rotor position in permanent magnet machine
- Index(es):
  - Date
  - Thread