[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Current orientation ?

- To: femm@yahoogroups.com
- Subject: Re: [femm] Current orientation ?
- From: David Meeker <dmeeker@ieee.org>
- Date: Tue, 27 Aug 2002 20:21:23 -0400
- References: <akfg8s+tgmb@eGroups.com>
- User-agent: Mozilla/5.0 (Windows; U; Windows NT 5.1; en-US; rv:1.0.0) Gecko/20020530

marsupiofr wrote:

> `Hi,
> when I apply a circuit property with a definition of a positive
> current, does this current flow "in to the page" or "out of the
> page" ?
> Thanks.
> `

For planar problems, positive current flows in the out-of-the-page direction. However, as a result of the orientation that I chose to display axisymmetric problems (e.g. as opposed to Quickfield), positive current must flow in the into-the-page direction for axisymmetric problems.
--
David Meeker

- References:
  - Current orientation ?
    - From: "marsupiofr" <marsupio@hotmail.com>

- Prev by Date: Re: [femm] Bug with showdensity, hidepoints and windowhide ?
- Next by Date: jiles-atherton model
- Previous by thread: Current orientation ?
- Next by thread: Bug with showdensity, hidepoints and windowhide ?
- Index(es):
  - Date
  - Thread