[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# [FEMM] Force Vs displacement of Magnet2.fem example

- To: femm@list.foster-miller.net
- Subject: [FEMM] Force Vs displacement of Magnet2.fem example
- From: Bhatti <bhatti@enveng.titech.ac.jp>
- Date: Thu, 23 Oct 2003 07:40:22 +0900
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: Finite Element Method Magnetics mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- Reply-to: Finite Element Method Magnetics mailing list <femm@list.foster-miller.net>

`Dear member`
`In example file of Magnet2.fem as the force vs displacement curve is changing from 0 to 2 cm gap with a value of about 8000N to 375N. How can i control this force what is the importance of this graph because current input is constant. if current is constant then the force must be constant. If any one know more about it please explain in detail. Thanks`
`Best personnel regards`

    Bhatti
    Master student
    Tokyo Institute of Technology

``

- Prev by Date: Re: [FEMM] Modeling multiple turn coils
- Next by Date: [FEMM] Magnetizing Inductance and Iron Resistance in Induction Machine
- Previous by thread: Re: [FEMM] Tape wound core modeling
- Next by thread: [FEMM] Magnetizing Inductance and Iron Resistance in Induction Machine
- Index(es):
  - Date
  - Thread