[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: inductance

- To: femm@yahoogroups.com
- Subject: Re: inductance
- From: tborzic@yahoo.com
- Date: Tue, 13 Nov 2001 21:20:26 -0000
- In-reply-to: <3BF15408.66033985@foster-miller.com>
- User-agent: eGroups-EW/0.82

    Thanks Dave, that was the clue,but I am still far from solution.
    My mistake is i did not describe my problem well.
    I am working on my graduate study (that why I translate
    manual:)). Part of my work is to prove that programs like femm
    (free) can replace old way of callculating numerical problems.
    Point is in precision and ability of solving different problems.
    I solved (ehm, femm did) all problems but one.
    thing is that I need to prove that in comparison with
    one-turn coil all other coils with n turns
    ( n=2,3,4,5...etc) have n^2 times larger inductance.
    Or, maybe, if 1 turn coil is not good for considering should
    I take 50 turns and 100 turns coil for comparison (altough,
    drawing 100 turns...huh)
    With file I attached earlier I can not achieve that.
    I assume it is because of dimensions of wire, which is
    neglected in "hand" callculations.
    So, any ideas? Explanations?
    Thanks
    Tomislav

- References:
  - Re: [femm] inductance
    - From: David Meeker <dmeeker@foster-miller.com>

- Prev by Date: Re: [femm] inductance - axisymmetric model
- Next by Date: Re: inductance - axisymmetric model
- Previous by thread: Re: [femm] inductance
- Next by thread: Inductance
- Index(es):
  - Date
  - Thread