[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# RES: [femm] High Temperature Magnet Wire (>240C)

- To: <femm@yahoogroups.com>
- Subject: RES: [femm] High Temperature Magnet Wire (>240C)
- From: "Paulo Valadares" <v2studio@terra.com.br>
- Date: Sat, 14 Jun 2003 17:34:59 -0300
- Disposition-notification-to: "Paulo Valadares" <v2studio@terra.com.br>
- Importance: Normal
- In-reply-to: <bce8eb+8j5i@eGroups.com>

    Hy David
    You can use Teflon coated wire.
    Ask for it in the manufacturer Kanthal Palm Coast in Florida
    Best Wishes
    Paulo Valadares
    São Paulo Brasil

    -----Mensagem original-----
    De: davidsde01 [mailto:davidsde01@netscape.net]
    Enviada em: sábado, 14 de junho de 2003 01:31
    Para: femm@yahoogroups.com
    Assunto: [femm] High Temperature Magnet Wire (>240C)

    I am in the process of designing a solenoid coil for use in a machine
    with a maximum operating temperature of 200C. At this operating
    temperature, I have a severe power constraint due to the 40C
    temperature rise over ambient that a class 240C wire will tolerate.

    Does anyone know of magnet wire rated in excess of 240C?

    I have heard of ceramic coated wire (can't afford it) and anodized
    aluminum wire (can't find it) that supposedly can handle much higher
    temperatures. Let me know what you think.

    Regards,

    Dan Davidson

    Your use of Yahoo! Groups is subject to http://docs.yahoo.com/info/terms/

    Esta mensagem foi verificada pelo E-mail Protegido Terra.
    Scan engine: VirusScan / Atualizado em 11/06/2003 / Versão: 1.3.13
    Proteja o seu e-mail Terra: http://www.emailprotegido.terra.com.br/

- References:
  - High Temperature Magnet Wire (>240C)
    - From: "davidsde01" <davidsde01@netscape.net>

- Prev by Date: High Temperature Magnet Wire (>240C)
- Next by Date: Re: [femm] (unknown)
- Previous by thread: High Temperature Magnet Wire (>240C)
- Next by thread: Re: [femm] High Temperature Magnet Wire (>240C)
- Index(es):
  - Date
  - Thread