[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Permanent Magnet Models.

- To: femm@egroups.com
- Subject: Permanent Magnet Models.
- From: Sebastia Jardi Estadella <sje@tinet.org>
- Date: Wed, 26 Apr 2000 13:16:47 -0700
- References: <8d9u2a+1s14@eGroups.com>

    Hi all:
    In my permanent magnet provider catalog I have Permeability in
    different
    units, for:
    Ferrite magnets: 1.35 mT/(kA/m) and 1.10 G/Oe
    Neodimium: 1.36 mT/(kA/m) and 1.08 G/Oe
    Samarium: 1.32 mT/(kA/m) and 1.05 G/Oe

    What unit system use FEMM for Permeability?

    For Coercivity, in the catalog I have Hcb (B=0) and Hcj (j=0). The
    correct value for the model is Hcb?

    Thank You.

    Sebastia Jardi Estadella
    mailto:sje@tinet.org
    http://www.tinet.org/~sje/index_en.htm

- References:
  - boundary conditions
    - From: strydah@cybertours.com

- Prev by Date: Re: [femm] Modelling a magnetometer
- Next by Date: Re: [femm] Permanent Magnet Models.
- Previous by thread: boundary conditions
- Next by thread: Re: [femm] boundary conditions
- Index(es):
  - Date
  - Thread