[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: boundary-conditions

- To: femm@yahoogroups.com
- Subject: Re: boundary-conditions
- From: "David Meeker" <dmeeker@ieee.org>
- Date: Mon, 01 Sep 2003 16:39:38 -0000
- In-reply-to: <20030831115135.12059.qmail@web14408.mail.yahoo.com>
- User-agent: eGroups-EW/0.82

    --- In femm@yahoogroups.com, Edgar Peralta <eperaltas@y...> wrote:
    > Hello everybody
    >
    > David, thank you for femm, it is great.
    >
    > I am trying to simulate an induction machine by
    > modeling a single-slot only. The model that I am using
    > is attached to this mail.
    >
    > If for any point x on edge AD corresponds a point y on
    > edge BC, how can I apply the boundary condition
    > Ay=Ax*exp(-j*alpha) along both edges?.
    >
    > Thanks in advance.
    >
    > Edgar

    The way that the program currently works, one can only apply periodic
    or antiperiodic boundary conditions for "linking" two edges together.
    This would correspond to your alpha=0 and alpha=Pi cases. You'd have
    to change the way that the periodic boundary condition is implemented
    in the source code to do an arbitrary angle. The changes to do this
    probably wouldn't be too extensive.

    Dave.
    --
    David Meeker
    dmeeker@ieee.org
    http://femm.berlios.de/dmeeker

- References:
  - boundary-conditions
    - From: Edgar Peralta <eperaltas@yahoo.com.mx>

- Prev by Date: Re: [femm] torque calculation
- Next by Date: Re: torque calculation
- Previous by thread: boundary-conditions
- Next by thread: Transformer Forward curent and magnetizing current
- Index(es):
  - Date
  - Thread