[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Area cross section problem

- To: femm@yahoogroups.com
- Subject: Area cross section problem
- From: "tano1938" <rgarritano@comcast.net>
- Date: Thu, 17 Apr 2003 16:12:28 -0000
- User-agent: eGroups-EW/0.82

    I don't seem to be getting the correct cross section area using the
    femmview block integrals. In the file "FRT_OLD.fem" selecting the
    magnet block and then block cross section area, I get an area of 1.16
    square inches. The cross section area of the magnet (diameter = 1.45
    inches) is really 1.651 square inches. I assume the cross section
    area is the area normal to the flux. Is that right? Also, what if a
    block has more than one cross section area like the outer housing in
    the same file. Where does femmview take the cross section?

    Thanks for your help.

- Follow-Ups:
  - Re: [femm] Area cross section problem
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: Re: Problem with my very first design
- Next by Date: Re: [femm] Area cross section problem
- Previous by thread: Re: [femm] Re: 12L14 Case Hardened BH Curve?
- Next by thread: Re: [femm] Area cross section problem
- Index(es):
  - Date
  - Thread