[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: Induction Motor in FEMM

- To: femm@yahoogroups.com
- Subject: Re: Induction Motor in FEMM
- From: "kbranbg" <kbran@vmei.acad.bg>
- Date: Fri, 13 Sep 2002 14:01:07 -0000
- In-reply-to: <6935AEC3B7B5D611803400306E1F0EE103B84F@sem.razvoj.com>
- User-agent: eGroups-EW/0.82

    --- In femm@y..., Lovrenc Gasparin <lovrencg@e...> wrote:
    > Hi!
    >
    > I have the same problem!
    >
    > <<brus.FEM>>
    >
    > The results are wrong! There is something wrong with frequency. If I
    > multiply the frequency by 10 the results will be quite good.
    >
    > Where is the problem?
    >
    > Please send me your model.
    >
    >
    > Lovrenc

    You must use the slip frequency of the rotor
    to compute the eddy currents in the rotor.
    So, specify the slip frequency as working
    frequency to FEMM and do not allow eddy currents
    in the stator.

- References:
  - RE: [femm] Induction Motor in FEMM
    - From: Lovrenc Gasparin <lovrencg@email.si>

- Prev by Date: RE: [femm] Where did I make the mistake?
- Next by Date: RE: [femm] Where did I make the mistake?
- Previous by thread: RE: [femm] Induction Motor in FEMM
- Next by thread: RE: [femm] Induction Motor in FEMM
- Index(es):
  - Date
  - Thread