[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] GO Material

- To: femm@egroups.com
- Subject: Re: [femm] GO Material
- From: dcm3c@aol.com
- Date: Wed, 24 May 2000 20:08:39 EDT

    In a message dated 5/22/00 10:18:26 AM Eastern Daylight Time, fnent@aol.com
    writes:

    > Can structures using Grain Oriented electrical steel be evaluated in
    > Femm? I would like to observe the difference in flux patterns with GO and
    > non-GO materials.

    Well, you can assign different permeabilites in different directions in femm.
    This might get you part of the way there. However, the model of saturation
    currently used in femm isn't elaborate enough to correctly model the
    difference between model grain-oriented and non-oriented materials in
    saturation.

    Dave.
    --
    http://members.aol.com/dcm3c

- Prev by Date: Re: [femm] motion-induced torque
- Next by Date: Re: [femm] GO Material
- Previous by thread: Re: [femm] motion-induced torque
- Next by thread: Re: [femm] GO Material
- Index(es):
  - Date
  - Thread