[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Triangle call unsuccessful

- To: femm@yahoogroups.com
- Subject: Triangle call unsuccessful
- From: "irishmist_ <djtim@worldnet.att.net>" <djtim@worldnet.att.net>
- Date: Wed, 05 Feb 2003 20:36:18 -0000
- User-agent: eGroups-EW/0.82

    David,

    I was having problems meshing an assembly created from a DXF import.
    I have found another situation (unexpected) where Triangle will not
    mesh the geometry. If the tolerance value for the DXF import is made
    too small the resulting geometry will not mesh. (At least in my case)

    My particular case is a PM motor of unusual construction. (Very high
    pole count and slots) There are many arc segments and I am making an
    assumption that this is related to the problem. If I left the
    tolerance at the default the problem meshed just fine.

    BTW thanks for making this software available.

    Dan

- Follow-Ups:
  - Re: [femm] Triangle call unsuccessful
    - From: Jiri Vecerka <vecerkaj@yahoo.com>

- Prev by Date: Again
- Next by Date: Re: [femm] Again
- Previous by thread: Re: [femm] Again
- Next by thread: Re: [femm] Triangle call unsuccessful
- Index(es):
  - Date
  - Thread