[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# lua scripting

- To: femm@yahoogroups.com
- Subject: lua scripting
- From: giovanni.bortolan@sogagroup.com
- Date: Thu, 18 Oct 2001 12:02:31 +0200

    Hi everybody

    In a Lua setgrid() is not available for preprocessor.
    Since i find comfortable switching from polar to cartesian coordinates and
    vice versa for adding nodes, is there a way to do this?
    I think about setgrid() for preprocessor or, better, something like
    addnodepolar(r, theta) and eventually selectnodepolar(r, theta).

    Another question.
    Is it possible to create a recording of the interaction with femm, in Lua?
    I mean something like a macro recording in Lua.
    In this way it would be very fast to set up a problem directly in Femm, and
    than manage modifications in Lua.

    _______________________________
    ing. G.Bortolan

    Sincro srl
    via Tezze, 3 loc. Cereda
    36073 Cornedo Vicentino (VI)
    Tel: (++39) 0445 450 500
    Fax: (++39) 0445 446 222
    e-mail: Giovanni.Bortolan@sogagroup.com
    tecnico.sincro@sogagroup.com

    REA 194515/VI
    Reg. Imp. 20968/VI 116
    P.IVA 01925820241

- Follow-Ups:
  - RE: [femm] lua scripting
    - From: "Robin Cornelius" <robin.cornelius@hirst-magnetics.com>

- Prev by Date: Boundary conditions of induction motor
- Next by Date: RE: [femm] lua scripting
- Previous by thread: Boundary conditions of induction motor
- Next by thread: RE: [femm] lua scripting
- Index(es):
  - Date
  - Thread