[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# New issues

- To: femm@yahoogroups.com
- Subject: New issues
- From: "marsupiofr" <marsupio@hotmail.com>
- Date: Tue, 27 Aug 2002 14:57:06 -0000
- User-agent: eGroups-EW/0.82

    Dave,

    in fact, after investigations, I encounter several issues concerning
    graphics outputs in FEMM 3.2 (error message when I create a bitmap in
    a LUA script,...). I installed the previous release (FEMM 3.1 of
    January 2002) and there are no problems any more. Do not know what
    really happens. All these issues have to be confirmed by other users.

    Yours Sincerely.

    PS1 : the LUA console is great to formerly test the scripts step-by-
    step

    PS2 : I'm dealing right now with a huge simulation where I calculate
    the mutual inductances between stator/rotor in a 3-phase squirrel
    cage induction machine (phase A supplied by a unit DC current and
    flux calculated through 2 adjacent rotor bars for instance). The
    rotation of the rotor is performed by a LUA script which moves the
    rotor part of a given step angle (for instance 1 degree). At each
    step, a picture of the postprocessor is taken (to be include later in
    a AVI file). That's how I encounter the above problems in FEMM 3.2

- Prev by Date: Bug with showdensity, hidepoints and windowhide ?
- Next by Date: [no subject]
- Previous by thread: Re: [femm] Bug with showdensity, hidepoints and windowhide ?
- Next by thread: [no subject]
- Index(es):
  - Date
  - Thread