[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# [Circuit Model]

- To: femm@yahoogroups.com
- Subject: [Circuit Model]
- From: "you se-ho" <sxy28@hotmail.com>
- Date: Fri, 28 Sep 2001 15:14:31
- Bcc:

`
To Dear All:`
`How are you?`

    Simulation (1) I define in the circuit define menu:
    circuit 1: +1A
    Circuit 2: +1A
    circuit 3: -2A (so, acts return ground.)

`Simulation (2) Circuit A: +1A
Circuit B :-1A (this is the return ground.)
then I assigned the "circuit A" to two traces. And I found the FEMM
altomatically divided the current half and half.`
`I check inductance and resistive loss. I expected them same, but now`
`Is there anybody knows the reason?`

    Thank you very much
    Sincerely,
    SE-HO YOU

``

    _________________________________________________________________
    Get your FREE download of MSN Explorer at http://explorer.msn.com/intl.asp

- Follow-Ups:
  - Re: [femm] [Circuit Model]
    - From: David Meeker <dmeeker@foster-miller.com>

- Prev by Date: Trouble with a 90° magnetic filter coil
- Next by Date: Re: [femm] [Circuit Model]
- Previous by thread: Re: [femm] Trouble with a 90° magnetic filter coil
- Next by thread: Re: [femm] [Circuit Model]
- Index(es):
  - Date
  - Thread