[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [FEMM] Reg : Coil Turns in serie/2conductors parallel

- To: FEMM mailing list <femm@list.foster-miller.net>
- Subject: Re: [FEMM] Reg : Coil Turns in serie/2conductors parallel
- From: Santiago Salamanca <santiago@salamanca.de>
- Date: Fri, 5 Mar 2004 19:21:42 +0100
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: FEMM mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- References: <200403041700.i24H0Dv3080937@fmi2.ncia.net> <4047F6E5.A530E690@bhelrnd.co.in>
- Reply-to: FEMM mailing list <femm@list.foster-miller.net>

Hi Prem Kumar, C

Thank you for your proposal, but i am trying to calculate with FEMM the losses for EACH conductor and not only the total losses of the coil, also the losses in 5*2=10 conductors, because the losses are very, very different from conductor to conductor. It is very important to calculate the losses from each conductor!!

The model is Axisymmetric.

Thank you

Santiago Salamanca

C.Prem Kumar schrieb am 05.03.2004:

> Hi Santiago,
> I understand you'd like to model a coil of FIVE turns carrying a current of 10,000Amps. I take it that the coil has two thick strands since you are also specific about 5000Amps per turn.

> If what I've understood is right this is the way to go about :

> 1. Represent the coil overall physical cross-sectional area in your model without bothering about the interturn space.
> 2. If the model is Axisymmetric assign the current value "5000*5*2" that is 50,000+ j0 as Total Current via the Circuit Properties. Do not forget to assign it a name.
> 3. If the model is 2D, you will have the coil represented as two sections. Via Circuit Properties assign +50,000+ j0 as the Total Current on the right-hand section. Give it a name. Assign -50,000+j0 on the other section. Give it a different name.
> I hope I've clarified your doubt !!

> Prem Kumar, C

> femm-request@list.foster-miller.net wrote:

> > Message: 3
> > Date: Wed, 3 Mar 2004 19:42:19 +0100
> > From: Santiago Salamanca <santiago@salamanca.de>
> > Subject: [FEMM] Coil Turns in serie/2conductors parallel
> > To: FEMM <femm@list.foster-miller.net>
> > Message-ID: <W.20040303194219.25A5.1.1DAD@post.strato.de>
> > Content-Type: text/plain; charset="iso-8859-1"

> > Dear Dr. David Meeker,
> > Hi all,
> > ?How to define a coil with turns in serie, but each turn has 2
> > conductos in parallel?

> > By Coil5Tparal i have defined a coil with 5 Turns in Serie, but
> > each Turn has 2 conductors
> > A conductor:18*10; Conductor-Isolation:4mm, Turn-Isolation 10mm.
> > The length of the coil is:5*18*2+5*4+4+100240mm.

> > The circuit current 10000 A, also 5000A/conductor as "serie"
> > ?How to define the conductors, as Group1 and Group2??Is that all
> > right?
> > ?Or how to define it?

> > Thank for you help

> > Santiago Salamanca

- Follow-Ups:
  - Re: [FEMM] Reg : Coil Turns in serie/2conductors parallel
    - From: "Fabio" <fmilanesi@tin.it>

- References:
  - [FEMM] Reg : Coil Turns in serie/2conductors parallel
    - From: "C.Prem Kumar" <prem@bhelrnd.co.in>

- Prev by Date: [FEMM] Reg : Coil Turns in serie/2conductors parallel
- Next by Date: Re: [FEMM] Reg : Coil Turns in serie/2conductors parallel
- Previous by thread: [FEMM] Reg : Coil Turns in serie/2conductors parallel
- Next by thread: Re: [FEMM] Reg : Coil Turns in serie/2conductors parallel
- Index(es):
  - Date
  - Thread