[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Femm releases 3.3 - 3.2

- To: femm@yahoogroups.com
- Subject: Femm releases 3.3 - 3.2
- From: "ac090960 <ac090960@yahoo.it>" <ac090960@yahoo.it>
- Date: Sun, 15 Dec 2002 11:31:12 -0000
- User-agent: eGroups-EW/0.82

    Hello,

    Making some trials with the new release 3.3 (downloaded today) on an
    AC axisymmetric geometry an error occurred during FKN execution: (On-
    edge lamination not supported in AC analyses).
    The strange is the same problem is running using the release 3.2.

    The problem to be solved is composed by a steel coil (Laminated
    parallel to z, to simulate a tape of steel wound as a coil) and a
    coaxial copper coil, the frequency is 50 Hz. The same happens
    imposing in the Lamination Attributes window the option: Laminated
    parallel to r (stacked steel disks problem).

    The only way to run the file on release 3.3 is to impose in the
    Lamination Attributes window the options: Not laminated or laminated
    in-plane.

    It would be very helpful to know why the difference in behaviour
    for the two releases (3.2 and 3.3) and if both releases can be used
    to solve such problem.

    Thanks in advance for reply

    Arnoldo.

- Follow-Ups:
  - Re: [femm] Femm releases 3.3 - 3.2
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: Re: [femm] Call to triangle unsucessful after import of DXF
- Next by Date: Re: [femm] Femm releases 3.3 - 3.2
- Previous by thread: Re: [femm] General question and/or proposition for the circuit property and global variable
- Next by thread: Re: [femm] Femm releases 3.3 - 3.2
- Index(es):
  - Date
  - Thread