[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# How to do a B or H "black box" generator in a perpendicular plan to the working

- To: femm@yahoogroups.com
- Subject: How to do a B or H "black box" generator in a perpendicular plan to the working
- From: "jire602000 <jire602000@yahoo.com>" <jire602000@yahoo.com>
- Date: Fri, 17 Jan 2003 19:53:07 -0000
- User-agent: eGroups-EW/0.82

    Hello every body,

    With the Prescribe A boundary condition, B or H can be imposed in
    the x y (r, z) 2D plan of the study . But how can I make it
    perpendicular to this plan ? I want it in the same direction as the
    current of the circuit property of a copper wire for example.

    This trick can also be achieved by having a current in a cooper wire
    running in the x y 2D plan and not in the perpendicular plan as usual
    .

    So , I need help and advise !

- Follow-Ups:
  - Re: [femm] How to do a B or H "black box" generator in a perpendicular plan to the working
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: Need BH curve for chromium steel
- Next by Date: Re: [femm] Need BH curve for chromium steel
- Previous by thread: RE: [femm] Need BH curve for chromium steel
- Next by thread: Re: [femm] How to do a B or H "black box" generator in a perpendicular plan to the working
- Index(es):
  - Date
  - Thread