[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# High Temperature Magnet Wire (>240C)

- To: femm@yahoogroups.com
- Subject: High Temperature Magnet Wire (>240C)
- From: "davidsde01" <davidsde01@netscape.net>
- Date: Sat, 14 Jun 2003 04:31:07 -0000
- User-agent: eGroups-EW/0.82

    I am in the process of designing a solenoid coil for use in a machine
    with a maximum operating temperature of 200C. At this operating
    temperature, I have a severe power constraint due to the 40C
    temperature rise over ambient that a class 240C wire will tolerate.

    Does anyone know of magnet wire rated in excess of 240C?

    I have heard of ceramic coated wire (can't afford it) and anodized
    aluminum wire (can't find it) that supposedly can handle much higher
    temperatures. Let me know what you think.

    Regards,

    Dan Davidson

- Follow-Ups:
  - RES: [femm] High Temperature Magnet Wire (>240C)
    - From: "Paulo Valadares" <v2studio@terra.com.br>
  - Re: [femm] High Temperature Magnet Wire (>240C)
    - From: "Richard Martin" <dick_martin@worldnet.att.net>

- Prev by Date: [no subject]
- Next by Date: RES: [femm] High Temperature Magnet Wire (>240C)
- Previous by thread: RE: [femm] (unknown)
- Next by thread: RES: [femm] High Temperature Magnet Wire (>240C)
- Index(es):
  - Date
  - Thread