[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# [FEMM] Accuracy error

- To: femm@list.foster-miller.net
- Subject: [FEMM] Accuracy error
- From: Dewald Pieterse <s99224055@tuks.co.za>
- Date: Mon, 26 Apr 2004 13:55:02 +0200
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: FEMM mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- Organization: University of Pretoria
- Reply-to: FEMM mailing list <femm@list.foster-miller.net>
- User-agent: Opera7.23/Linux M2 build 518

`Femm gives the following error when I want to mesh my problem, attached is the fem document. What am I doing wrong or is there a setting that I need to change??`

    Error:  Ran out of precision at (145.840386091, 120.550876183).
    I attempted to split a segment to a smaller size than can
      be accommodated by the finite precision of floating point
      arithmetic.
    Try increasing the area criterion and/or reducing the minimum
      allowable angle so that tiny triangles are not created.

``
`Thanks`
`Dewald`

    --
    Using M2, Opera's revolutionary e-mail client: http://www.opera.com/m2/

Attachment: `Halbachmotor.FEM`
Description: Binary data

- Follow-Ups:
  - Re: [FEMM] Accuracy error
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: Rif: Re: [FEMM] lua to output B field
- Next by Date: [FEMM] [cogging torque problem???]
- Previous by thread: Rif: Re: [FEMM] lua to output B field
- Next by thread: Re: [FEMM] Accuracy error
- Index(es):
  - Date
  - Thread