[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Calculation of force

- To: femm@yahoogroups.com
- Subject: Re: [femm] Calculation of force
- From: agnaldo@if.ufrj.br
- Date: Wed, 14 Aug 2002 14:31:05 -0300 (BRT)
- In-reply-to: <00c901c242d4$7b094420$027314ac@axp.valm.army.sk>
- References: <00c901c242d4$7b094420$027314ac@axp.valm.army.sk>
- User-agent: IMP/PHP IMAP webmail program 2.2.7

    Hi.
    We are having the same kind of problem: the force value calculated once in a
    position isn't the same when calculated at the same position using LUA script.
    Can anybody help?

    > Hello femm group.
    > I have a problem. I have simulation force effects between feromagnetic
    > core and coil in the electromagnet. This simulation I define as
    > axisimetric problem. The force is calculation by line integral (f =
    > lineintegral(3)) along the contour for different position of
    > feromagnetic core. When I made control estimation by post processor
    > (without lua script) I was found different results. In my opinoin the
    > results calculation by line integral are not right because theoretical
    > assumption is other. I don't know where I make errors.
    >
    > Thanks
    > Roman Beresik
    >

- Follow-Ups:
  - Re: [femm] Calculation of force
    - From: David Meeker <dmeeker@ieee.org>
  - Re: [femm] Calculation of force
    - From: David Meeker <dmeeker@ieee.org>

- References:
  - Calculation of force
    - From: "Roman Beresik" <beresikr@valm.sk>

- Prev by Date: saturable reactor
- Next by Date: Re: [femm] Calculation of force
- Previous by thread: Calculation of force
- Next by thread: Re: [femm] Calculation of force
- Index(es):
  - Date
  - Thread