[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Intrinsic and Normal Hc??

- To: femm@yahoogroups.com
- Subject: Re: [femm] Intrinsic and Normal Hc??
- From: David Meeker <dmeeker@foster-miller.com>
- Date: Wed, 08 Oct 2003 07:54:07 -0400
- In-reply-to: <blvpbr+ufm1@eGroups.com>
- References: <blvpbr+ufm1@eGroups.com>
- User-agent: Mozilla/5.0 (Windows; U; Windows NT 5.1; en-US; rv:1.4; MultiZilla v1.5.0.2d) Gecko/20030624

`ahmad_m_eid wrote:`

> `Dear all`
> `I have a confusion when I simulate the permanent magnet in femm.`

>     In most data sheets I have about Nd-Fe-B magnets, there are two
>     values for the coercive force (Hc), intrinsic and normal values.

>     My question is which one is used to simulate the permanent magnet in
>     femm?

> `any one knows sheet data reference for Nd-Fe-B magnet will be good.`
> `thanks you all`
> `ahmad`

`
The Hc that you enter as a material property in FEMM is the normal Hc.`
`The "normal coercivity"is the applied field intensity required to bring the flux density to zero inside the magnet. The "intrinsic coercivity," Hci, is the applied field intensity required to reverse the direction of the material's magnetization (i.e. to "break" the magnet). There is a nice page about all this at: http://www.magnetweb.com/Sect1C.htm`

    Dave.
    --

`David Meeker
Senior Engineer
Foster-Miller, Inc.
350 Second Avenue
Waltham, MA 02451-1196
781-684-4070
781-890-3489 (fax)
dmeeker@foster-miller.com`
``
``

- References:
  - Intrinsic and Normal Hc??
    - From: "ahmad_m_eid" <ahmad_m_eid@yahoo.com>

- Prev by Date: Intrinsic and Normal Hc??
- Next by Date: Change of address for FEMM website
- Previous by thread: Intrinsic and Normal Hc??
- Next by thread: Change of address for FEMM website
- Index(es):
  - Date
  - Thread