[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] GO Material

- To: femm@egroups.com
- Subject: Re: [femm] GO Material
- From: fnent@aol.com
- Date: Wed, 24 May 2000 20:54:12 EDT

    In a message dated 05/24/2000 7:25:28 PM Central Daylight Time, dcm3c@aol.com
    writes:

    <<
    > Can structures using Grain Oriented electrical steel be evaluated in
    > Femm? I would like to observe the difference in flux patterns with GO and
    > non-GO materials.

    Well, you can assign different permeabilites in different directions in
    femm.
    This might get you part of the way there. However, the model of saturation
    currently used in femm isn't elaborate enough to correctly model the
    difference between model grain-oriented and non-oriented materials in
    saturation.

    Dave. >>

    Dave,
    Thanks for the reply. I tried assigning the x-y permeabilities but
    the answer was not affected as much as it should have been as your answer
    suggests.

    Thank you,
    Joseph Pijanowski

- Follow-Ups:
  - Re: [femm] GO Material
    - From: David Meeker <dmeeker@foster-miller.com>

- Prev by Date: Re: [femm] GO Material
- Next by Date: Re: [femm] motion-induced torque
- Previous by thread: Re: [femm] GO Material
- Next by thread: Re: [femm] GO Material
- Index(es):
  - Date
  - Thread