[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Circuits in FEMM

- To: femm@yahoogroups.com
- Subject: Circuits in FEMM
- From: frank.e.lenning@boeing.com
- Date: Tue, 04 Sep 2001 17:56:06 -0000
- User-agent: eGroups-EW/0.82

    How does the circuits feature in FEMM work for multiple conductors?
    Let's say I have two conductors of different materials that I define
    with Circuits to be carrying a total current of 1 amp together. How
    does FEMM solve this problem? Does it iteratively solve the problem
    by choosing different deltaV's for each conductor until it gets the
    right total current or is there some easier way that it uses to set
    the deltaV's? It appears to get the right answer, I'm just trying to
    understand how.

- Follow-Ups:
  - Re: [femm] Circuits in FEMM
    - From: David Meeker <dmeeker@foster-miller.com>

- Prev by Date: Re: LUA pause command
- Next by Date: RE: [femm] script convention
- Previous by thread: Re: [femm] Help
- Next by thread: Re: [femm] Circuits in FEMM
- Index(es):
  - Date
  - Thread