[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: External Load in FEMM

- To: femm@yahoogroups.com
- Subject: Re: External Load in FEMM
- From: "David Meeker" <dmeeker@ieee.org>
- Date: Fri, 03 Oct 2003 13:46:10 -0000
- In-reply-to: <blfu1p+uae9@eGroups.com>
- User-agent: eGroups-EW/0.82

    --- In femm@yahoogroups.com, "ahmad_m_eid" <ahmad_m_eid@y...> wrote:
    > Dear all
    >
    > I think in something may be good, if it is possibles in femme. I work
    > on linear generator, there is an induced emf on stator terminals. I
    > want to simulate an external load to the generator terminals, so one
    > can examine some of the properties of the designed generator. If it
    > is possible, please explain how?
    >
    > any idea will be good.
    >
    > thanx all
    >
    > ahmad

    The program currently doesn't have a coupling to external circuits.
    The way that you'd proceed is to deduce the induced voltage on the
    terminals through computations of flux linkage.

    Dave.

- References:
  - External Load in FEMM
    - From: "ahmad_m_eid" <ahmad_m_eid@yahoo.com>

- Prev by Date: Re: ac current
- Next by Date: Calculation of screen current
- Previous by thread: External Load in FEMM
- Next by thread: ac current
- Index(es):
  - Date
  - Thread