[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: Temperature dependence of PM materials

- To: femm@yahoogroups.com
- Subject: Re: Temperature dependence of PM materials
- From: "fj_emtc" <fije29@sol.dk>
- Date: Fri, 04 Oct 2002 06:29:28 -0000
- In-reply-to: <ani7lj+8c04@eGroups.com>
- User-agent: eGroups-EW/0.82

    --- In femm@y..., "David Meeker" <dcm3c@e...> wrote:
    (btw, is Thermoflux an example of such a material?)
    >
    > Dave.

    Thermoflux is a nickel-iron alloy with around 30% nickel. Changing
    the content and heat treatment changes the Curie point.
    (30°-120°C).
    Se Soft Magnetic Material from Vacuumschmelze ISBN 0-85501-263-3 or
    go to www.vacuumschmelze.com and search for Thermoflux

    Finn Jensen

- Follow-Ups:
  - Re: [femm] Re: Temperature dependence of PM materials
    - From: David Meeker <dmeeker@ieee.org>

- References:
  - Re: Temperature dependence of PM materials
    - From: "David Meeker" <dcm3c@earthlink.net>

- Prev by Date: RE: [femm] Re: Temperature dependence of PM materials
- Next by Date: Re: [femm] Re: Temperature dependence of PM materials
- Previous by thread: Re: [femm] Re: Temperature dependence of PM materials
- Next by thread: Re: [femm] Re: Temperature dependence of PM materials
- Index(es):
  - Date
  - Thread