[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Material proprietes: magnet

- To: <femm@yahoogroups.com>
- Subject: Material proprietes: magnet
- From: "TMax" <mrtycho@libero.it>
- Date: Sun, 20 Jul 2003 00:06:57 +0200
- References: <bf69hl+9nh2@eGroups.com> <00a201c34d63$621a7cf0$5a5e623e@tmdesk>

    Preprocessor
    As showed in the manual, a permanent magnet is described by an Hc value that
    shift remain values to the origin.
    In linear relationship a relative permeability is set.(obtained by
    Br/Hc/air_permeability?!)

    Postprocessor
    If i check any points in a magnet, result value of induction correspond to
    |H|-Hc??!

    Thanks in advance.
    TMax

- Follow-Ups:
  - Re: [femm] Material proprietes: magnet
    - From: David Meeker <dmeeker@ieee.org>

- References:
  - Re: How calculate distribution and value of EMF?
    - From: "masteringmatlab" <masteringmatlab@yahoo.com>
  - Re: [femm] Re: How calculate distribution and value of EMF?
    - From: "TMax" <mrtycho@libero.it>

- Prev by Date: Re: [femm] Induction Motor Tourqe Calculation
- Next by Date: Re: [femm] Material proprietes: magnet
- Previous by thread: Re: [femm] Re: How calculate distribution and value of EMF?
- Next by thread: Re: [femm] Material proprietes: magnet
- Index(es):
  - Date
  - Thread