[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Re: Current

- To: femm@yahoogroups.com
- Subject: Re: [femm] Re: Current
- From: Keith Gregory <k.gregory@lboro.ac.uk>
- Date: Wed, 24 Jul 2002 08:15:04 +0100
- In-reply-to: <3D3D5EDA.9040108@ieee.org>
- References: <ahgh7h+q70o@eGroups.com> <5.1.0.14.0.20020723080648.00aa9230@staff-mailin.lboro.ac.uk>

>     Yes, that's right--the current density that you assign is a "source
>     current density" which would be the same as conductivity*voltage
>     gradient (at least for regions with a nonzero conductivity...) To force
>     a particular net current on a conductive region regardless of frequency,
>     you have to use the "circuit" properties to do it.

> `Dave.`

`
I get it. See Brian I told you we should ask Dave!`
`Keith.`
``

- References:
  - Re: Current
    - From: "brian_hawes" <b.hawes1@physics.ox.ac.uk>
  - Re: [femm] Re: Current
    - From: Keith Gregory <k.gregory@lboro.ac.uk>
  - Re: [femm] Re: Current
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: RE: How to use "Copy as Metafile"
- Next by Date: Induction Machine in FEMM
- Previous by thread: Re: [femm] Re: Current
- Next by thread: Force using LUA
- Index(es):
  - Date
  - Thread