[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: inductance - revised axisymmetric model

- To: femm@yahoogroups.com
- Subject: Re: inductance - revised axisymmetric model
- From: tborzic@yahoo.com
- Date: Wed, 14 Nov 2001 19:47:04 -0000
- In-reply-to: <F197BWVvPfpXJ6PxbMP0000a435@hotmail.com>
- User-agent: eGroups-EW/0.82

    thanx Jim, I hope that will do with The Professor.
    I have one more question..

    As you may see, inductance is generally my problem.
    Currently i am trying to solve inductance between
    two reactangular conductors, infinite lenghth, paralell.
    they are standing like this - II.
    Numerically, inductance for such case is:

    L=(2*mi0/h)*(b+a/3)

    where h-heighth,2b distance between conductors (not
    between theirs centers), and a width.
    so if a=0.2cm, b=0.8cm (2b = distance 1.6cm),h=2.2cm
    L=9.89 e-7 H/m, while femm allways returns half of that value.
    I applied 1A current for easier computing.
    so, where is mistake?
    thanks
    tomislav

- References:
  - Re: [femm] Re: inductance - revised axisymmetric model
    - From: "Jim in_Dallas" <jim271@hotmail.com>

- Prev by Date: Re: [femm] Re: inductance - revised axisymmetric model - fem files attached
- Next by Date: Re: [femm] Re: inductance - parallel strips
- Previous by thread: Re: [femm] Re: inductance - revised axisymmetric model
- Next by thread: Re: [femm] Re: inductance - revised axisymmetric model
- Index(es):
  - Date
  - Thread