[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Re: Temperature dependence of PM materials

- To: femm@yahoogroups.com
- Subject: Re: [femm] Re: Temperature dependence of PM materials
- From: David Meeker <dmeeker@ieee.org>
- Date: Fri, 04 Oct 2002 09:23:31 -0400
- References: <anjcg8+rchc@eGroups.com>
- User-agent: Mozilla/5.0 (Windows; U; Windows NT 5.1; en-US; rv:1.1) Gecko/20020826

`fj_emtc wrote:`

>     --- In femm@y..., "David Meeker" <dcm3c@e...> wrote:
>     (btw, is Thermoflux an example of such a material?)
>     >
>     > Dave.

>     Thermoflux is a nickel-iron alloy with around 30% nickel. Changing
>     the content and heat treatment changes the Curie point.
>     (30°-120°C).
>     Se Soft Magnetic Material from Vacuumschmelze ISBN 0-85501-263-3 or
>     go to www.vacuumschmelze.com and search for Thermoflux

> `
> Finn Jensen`

`
Ok--now I've found it. Thanks again for the pointers--I really appreciate them.`

    Dave.
    --
    David Meeker <http://femm.berlios.de/dmeeker>

- References:
  - Re: Temperature dependence of PM materials
    - From: "fj_emtc" <fije29@sol.dk>

- Prev by Date: Re: [femm] Re: Temperature dependence of PM materials
- Next by Date: Re: Temperature dependence of PM materials
- Previous by thread: Re: Temperature dependence of PM materials
- Next by thread: Re: [femm] Temperature dependence of PM materials
- Index(es):
  - Date
  - Thread