[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# [femm] torque calculation

- To: "'femm mailing list'" <femm@eGroups.com>
- Subject: [femm] torque calculation
- From: Tecnico <tecnico@sincro.it>
- Date: Thu, 16 Mar 2000 12:42:45 +0100
- Delivered-to: listsaver-of-femm@egroups.com
- Delivered-to: listsaver-egroups-femm@eGroups.com
- List-archive: <http://www.egroups.com/group/femm/>
- List-help: <http://www.egroups.com/group/femm/info.html>, <mailto:femm-help@egroups.com>
- List-unsubscribe: <mailto:femm-unsubscribe@egroups.com>
- Mailing-list: contact femm-owner@egroups.com
- Reply-to: femm@egroups.com

    Thank you Dave,

    I was taking relative permeability instead of absolute permeability.
    Now torque is correct.

    G.Bortolan

- Prev by Date: [femm] Re: No Subject / Materials....
- Next by Date: [femm] part motor stator modeling???
- Previous by thread: [femm] Re: No Subject / Materials....
- Next by thread: [femm] part motor stator modeling???
- Index(es):
  - Date
  - Thread