[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# RE: [femm] torque calculation example

- To: <femm@yahoogroups.com>
- Subject: RE: [femm] torque calculation example
- From: "Juan Tapia" <jtapia@die.udec.cl>
- Date: Wed, 19 Mar 2003 16:47:50 -0400
- Importance: Normal
- In-reply-to: <3E78D46F.8040400@plix.com>

Noe it works!!...gracias! Juan A. Tapia -----Mensaje original----- De: Dave Squires [mailto:djsquires@plix.com] Enviado el: Miércoles, 19 de Marzo de 2003 16:35 Para: femm@yahoogroups.com Asunto: Re: [femm] torque calculation example `You must select the red line contour button on the left top` `first then left click on each point definingthe contour` `clockwise starting on any point.` `You must have just clicked on the contour line.` `DRS` `Juan Tapia wrote:` `> I?m sorry?but It didn?t work. I solved the problem, got the flux lines,` `> but when I try to click on` `> the center contour line. It is not selected? What I did wrong?` `>` `>` `>` `> Juan` `>` `>` `>` `>` `>` `>` `>` `> -----Mensaje original-----` `> De: Dave Squires [mailto:djsquires@plix.com]` `> Enviado el: Miércoles, 19 de Marzo de2003 14:28` `> Para: femm@yahoogroups.com` `> Asunto: Re: [femm] torque calculation example` `>` `>` `>` `> Here is a simple 2-pole motor example.` `> Juan,` `> Here is a very simple example.` `> There are other ways, of course, but maybe` `> this is good enough?` `>` `> No special boundary conditions are used.` `> The mesh is 0.02" between the rotor and stator` `> magnets. Units are inches.` `>` `> Once simulated use FEMMVIEW then left click on` `> the center contour line between the rotor and` `> stator magnets going clockwise.` `> Then click on the integrate->torque` `> from stress tensor selection.` `>` `> The gap is large to make it simple and so it` `> runs fast. I used version 3.2.` `>` `> I hope this helps.` `>` `> DRS` `>` `> penquista66 wrote:` `>> Hi Femm people` `>>` `>> I'm wondering if anyone can send a simple torque example calculation.` `>> I'm teaching an electromechanical energy conversion class and I'll be` `>> very interested to show to my students the procedure to calculate` `>> torque using FEMM with a simple example.` `>>` `>> Thanks` `>>` `>> Juan A.` `>>` `>>` `>>` `>>` `>>` `>>` `>> Your use of Yahoo! Groups is subject to http://docs.yahoo.com/info/terms/` `>>` `>>` `>>` `>` `>` `>` `> Your use of Yahoo! Groups is subject tothe Yahoo! Terms of Service` `> <http://docs.yahoo.com/info/terms/>.` `>` `>` `>` `> Yahoo! Groups Sponsor` `> <http://rd.yahoo.com/M=245314.3072841.4397732.2848452/D=egroupweb/S=1705083663:HM/A=1495890/R=0/*http://www.netbizideas.com/yheb42` `> >` `>` `>` `> Your use of Yahoo! Groups is subject tothe Yahoo! Terms of Service` `> <http://docs.yahoo.com/info/terms/>.` `Your use of Yahoo! Groups is subject to the Yahoo! Terms of Service.`

- Follow-Ups:
  - Re: [femm] torque calculation example
    - From: Dave Squires <djsquires@plix.com>

- References:
  - Re: [femm] torque calculation example
    - From: Dave Squires <djsquires@plix.com>

- Prev by Date: Re: [femm] question about makeplot()
- Next by Date: Re: [femm] torque calculation example
- Previous by thread: Re: [femm] torque calculation example
- Next by thread: Re: [femm] torque calculation example
- Index(es):
  - Date
  - Thread