[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Hang-up questions

- To: femm@yahoogroups.com
- Subject: Re: [femm] Hang-up questions
- From: Tom Hansen <tomh@sonic.net>
- Date: Mon, 22 Apr 2002 13:39:04 -0700
- References: <000001c1c5f1$122b43a0$0200a8c0@hirstmagnetics> <3CBFE604.42DB3CB0@gds-sistemas.com> <3CC412F2.30604@ieee.org>

    Hi Dave:

    I have been using this great program for awhile and often it works
    without hassles but occasionally when I import a dxf file there are
    small glitches. Usually the glitches are: double points, unconnected
    paths or very small areas of overlap. Sometimes these show up when
    doing the mesh, other times during the analysis where it will just hang
    and not signal an error. Is there a portion of the program that could
    do a "prior to run" error check that would flag these types of errors or
    log a snags list?

    Many Thanks,

    Tom

- Follow-Ups:
  - Re: [femm] Hang-up questions
    - From: David Meeker <dmeeker@ieee.org>

- References:
  - RE: [femm] savebitmap error
    - From: "Robin Cornelius" <robin.cornelius@hirst-magnetics.com>
  - Lua questions
    - From: GDS <gds@gds-sistemas.com>
  - Re: [femm] Lua questions
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: Minor documentation change
- Next by Date: harmonic analysis
- Previous by thread: Re: [femm] Lua questions
- Next by thread: Re: [femm] Hang-up questions
- Index(es):
  - Date
  - Thread