[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: Can femm model this?

- To: femm@yahoogroups.com
- Subject: Re: Can femm model this?
- From: "wigstonmagna" <andrew_ppp@hotmail.com>
- Date: Thu, 31 Jul 2003 01:16:50 -0000
- In-reply-to: <3F286B73.1050401@ieee.org>
- User-agent: eGroups-EW/0.82

    wigstonmagna wrote:
    I want to simulate a coil placed between two flat parallel metal
    plates, with the coil's long axis parallel to the plates. I want to
    electrically connect the inductance in parallel with the capacitor
    (the plates) and drive the assembly at AC.
    Can this be constructed?
    -Andrew

    David replied:
    Problems that FEMM can simulate have to be either axially symmetric
    (e.g. a solenoid, speaker driver, etc.) or approximated as planar
    (e.g. many types of motors). Although your coil may be axisymmetric,
    the entire arrangement isn't axisymmetric--you can't model it directly
    with FEMM.

    How about planar mode? Will a 2D slice work?

- Follow-Ups:
  - Re: [femm] Re: Can femm model this?
    - From: "H.Hasper" <h.Hasper@fwn.rug.nl>
  - Re: Can femm model this?
    - From: "wigstonmagna" <andrew_ppp@hotmail.com>

- References:
  - Re: [femm] Can femm model this?
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: Re: [femm] Can femm model this?
- Next by Date: Re: [femm] Re: Can femm model this?
- Previous by thread: Re: [femm] Can femm model this?
- Next by thread: Re: [femm] Re: Can femm model this?
- Index(es):
  - Date
  - Thread